
(rules PCB devBoard
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 6805)
    (layer_rule F.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.4)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 1.7)
    )
  )
  (rule
    (width 200.0)
    (clear 150.2)
    (clear 100.0 (type smd_to_turn_gap))
    (clear 200.2 (type default_Power))
    (clear 37.6 (type smd_smd))
    (clear 200.2 (type smd_Power))
    (clear 200.2 (type "kicad_default"_Power))
    (clear 200.2 (type Power_Power))
  )
  (padstack "Via[0-1]_600:400_um"
    (shape
      (circle F.Cu 600.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 600.0 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_600:400_um" "Via[0-1]_600:400_um" default
  )
  (via 
    "Via[0-1]_600:400_um-kicad_default" "Via[0-1]_600:400_um" "kicad_default"
  )
  (via 
    "Via[0-1]_600:400_um-Power" "Via[0-1]_600:400_um" Power
  )
  (via_rule
    default "Via[0-1]_600:400_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_600:400_um-kicad_default"
  )
  (via_rule
    Power "Via[0-1]_600:400_um-Power"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 200.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    "Net-(C2-Pad1)" "Net-(C5-Pad2)" "Net-(C6-Pad2)" "Net-(D1-Pad2)" D5 D6 D7 D8
    D9 D10 D11 D12 D13 RST Rx Tx
    WS2812B A5 A4 A3 A2 A1 A0 "Net-(LED1-Pad4)"
    "Net-(Q1-Pad1)" "Net-(Q2-Pad1)" "Net-(R1-Pad2)" "Net-(R4-Pad2)"
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 200.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class Power
    Vin GND +3V3 VCC T01 T02
    (clearance_class Power)
    (via_rule Power)
    (rule
      (width 400.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)