
(rules PCB TestDriverV1
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 4735)
    (layer_rule F.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.4)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 1.7)
    )
  )
  (rule
    (width 250.0)
    (clear 200.2)
    (clear 125.0 (type smd_to_turn_gap))
    (clear 50.0 (type smd_smd))
  )
  (padstack "Via[0-1]_800:400_um"
    (shape
      (circle F.Cu 800.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 800.0 0.0 0.0)
    )
    (attach off)
  )
  (padstack "Via[0-1]_1000:600_um"
    (shape
      (circle F.Cu 1000.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 1000.0 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_800:400_um" "Via[0-1]_800:400_um" default
  )
  (via 
    "Via[0-1]_1000:600_um" "Via[0-1]_1000:600_um" default
  )
  (via 
    "Via[0-1]_800:400_um-kicad_default" "Via[0-1]_800:400_um" "kicad_default"
  )
  (via 
    "Via[0-1]_1000:600_um-kicad_default" "Via[0-1]_1000:600_um" "kicad_default"
  )
  (via 
    "Via[0-1]_800:400_um-Power" "Via[0-1]_800:400_um" Power
  )
  (via 
    "Via[0-1]_1000:600_um-Power" "Via[0-1]_1000:600_um" Power
  )
  (via_rule
    default "Via[0-1]_800:400_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_800:400_um-kicad_default"
  )
  (via_rule
    Power "Via[0-1]_1000:600_um-Power"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 250.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    "Net-(C13-Pad1)" "Net-(C14-Pad1)" "Net-(C15-Pad1)" "Net-(C16-Pad1)" "Net-(JP5-Pad3)" "Net-(JP6-Pad3)" "Net-(R1-Pad2)" "Net-(R1-Pad1)"
    "Net-(R2-Pad1)" "Net-(R3-Pad1)" "Net-(R10-Pad2)" "Net-(R4-Pad1)" "Net-(R11-Pad2)" "Net-(R5-Pad1)" "Net-(R6-Pad1)" "Net-(R12-Pad2)"
    "Net-(R7-Pad1)" "Net-(R8-Pad1)" "Net-(R9-Pad1)" "Net-(R10-Pad1)" "Net-(R11-Pad1)" "Net-(R12-Pad1)"
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 250.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class Power
    GND "Net-(C1-Pad1)" "Net-(C2-Pad1)" "Net-(C3-Pad1)" "Net-(C4-Pad1)" VPSU01 VPSU02 VPSU03
    VPSU04 "Net-(D1-Pad1)" "Net-(D2-Pad1)" "Net-(D3-Pad1)" "Net-(D4-Pad1)" LED01 LED02 "Net-(J4-Pad1)"
    RawVoltage "Net-(JP5-Pad2)" vari01 vari02 "Net-(JP6-Pad2)" VDRIVER01 VDRIVER02 VDRIVER04
    VDRIVER03
    (clearance_class Power)
    (via_rule Power)
    (rule
      (width 1200.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)