(export (version D)
  (design
    (source /home/hendrik/Schreibtisch/FilmLED/TestDriverV1/TestDriverV1.sch)
    (date "Mo 24 Sep 2018 17:02:40 CEST")
    (tool "Eeschema 5.0.0")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title TestDriver)
        (company)
        (rev "Rev 1")
        (date 2018-09-23)
        (source TestDriverV1.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U5)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A1BC))
    (comp (ref C9)
      (value "47 µF 16V")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A30D))
    (comp (ref C13)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A4B2))
    (comp (ref R1)
      (value "0,11 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A521))
    (comp (ref D1)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A689))
    (comp (ref L1)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A6E3))
    (comp (ref U1)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7E9F1))
    (comp (ref C1)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7EB69))
    (comp (ref C5)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7EC87))
    (comp (ref SW1)
      (value SW_DIP_x03)
      (footprint Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x03) (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA8443A))
    (comp (ref R9)
      (value "0,165 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA85013))
    (comp (ref R2)
      (value "0,33 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA85055))
    (comp (ref J4)
      (value PowerIn)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA8AAE5))
    (comp (ref U6)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4B1))
    (comp (ref C10)
      (value "47 µF 16V")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4B7))
    (comp (ref C14)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4BD))
    (comp (ref R3)
      (value "0,11 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4C3))
    (comp (ref D2)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4C9))
    (comp (ref L2)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4CF))
    (comp (ref U2)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4E7))
    (comp (ref C2)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4ED))
    (comp (ref C6)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB4F3))
    (comp (ref SW2)
      (value SW_DIP_x03)
      (footprint Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x03) (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB522))
    (comp (ref R10)
      (value "0,165 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB528))
    (comp (ref R4)
      (value "0,33 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACB52E))
    (comp (ref U7)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFB79))
    (comp (ref C11)
      (value "47 µF 16V")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFB7F))
    (comp (ref C15)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFB85))
    (comp (ref R5)
      (value "0,11 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFB8B))
    (comp (ref D3)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFB91))
    (comp (ref L3)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFB97))
    (comp (ref U3)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFBAF))
    (comp (ref C3)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFBB5))
    (comp (ref C7)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFBBB))
    (comp (ref SW3)
      (value SW_DIP_x03)
      (footprint Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x03) (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFBEA))
    (comp (ref R11)
      (value "0,165 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFBF0))
    (comp (ref R6)
      (value "0,33 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFBF6))
    (comp (ref U8)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC2C))
    (comp (ref C12)
      (value "47 µF 16V")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC32))
    (comp (ref C16)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC38))
    (comp (ref R7)
      (value "0,11 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC3E))
    (comp (ref D4)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC44))
    (comp (ref L4)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC4A))
    (comp (ref U4)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC62))
    (comp (ref C4)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC68))
    (comp (ref C8)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC6E))
    (comp (ref SW4)
      (value SW_DIP_x03)
      (footprint Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x03) (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFC9D))
    (comp (ref R12)
      (value "0,165 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFCA3))
    (comp (ref R8)
      (value "0,33 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFCA9))
    (comp (ref JP7)
      (value LED01_Select)
      (footprint Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NC_Dual) (description "Dual Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAF848B))
    (comp (ref JP8)
      (value LED02_Select)
      (footprint Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NC_Dual) (description "Dual Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAF85F3))
    (comp (ref JP1)
      (value PSU01)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, generic, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB805E1))
    (comp (ref JP2)
      (value PSU02)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, generic, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB9EED9))
    (comp (ref JP3)
      (value PSU03)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, generic, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB9F143))
    (comp (ref JP4)
      (value PSU04)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, generic, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB9F471))
    (comp (ref JP5)
      (value "PSU 1+2")
      (footprint Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NC_Dual) (description "Dual Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BBFDD5C))
    (comp (ref JP6)
      (value "PSU 1+2")
      (footprint Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NC_Dual) (description "Dual Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC52749))
    (comp (ref J2)
      (value V01)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCA9F08))
    (comp (ref J3)
      (value V02)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCAA3AD))
    (comp (ref J1)
      (value toLED)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x03_Male) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCAA457))
    (comp (ref SW5)
      (value MainSW)
      (footprint w_switch:switch_100sp5)
      (libsource (lib Switch) (part SW_DPST_x2) (description "Single Pole Single Throw (SPST) switch, separate symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD86151))
    (comp (ref RV3)
      (value fix01)
      (footprint w_smd_resistors:trim_bourns_3214j)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA923B6))
    (comp (ref RV4)
      (value pot01)
      (footprint Potentiometer_THT:Potentiometer_Piher_T-16H_Single_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA92935))
    (comp (ref RV5)
      (value fix02)
      (footprint w_smd_resistors:trim_bourns_3214j)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA931A1))
    (comp (ref RV1)
      (value pot02)
      (footprint Potentiometer_THT:Potentiometer_Piher_T-16H_Single_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA933BB))
    (comp (ref RV7)
      (value pot03)
      (footprint Potentiometer_THT:Potentiometer_Piher_T-16H_Single_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA93583))
    (comp (ref RV6)
      (value fix03)
      (footprint w_smd_resistors:trim_bourns_3214j)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA93908))
    (comp (ref RV8)
      (value fix04)
      (footprint w_smd_resistors:trim_bourns_3214j)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA93C37))
    (comp (ref RV2)
      (value pot04)
      (footprint Potentiometer_THT:Potentiometer_Piher_T-16H_Single_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA94004)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Jumper)
      (description "Jumper, generic, normally closed")
      (docs ~)
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Jumper_NC_Dual)
      (description "Dual Jumper, normally closed")
      (docs ~)
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Dual))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_POT)
      (description Potentiometer)
      (docs ~)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) R_POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Driver_LED) (part AMC7150)
      (description "1.5A POWER LED DRIVER")
      (docs https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) AMC7150))
      (pins
        (pin (num 1) (name VCC) (type input))
        (pin (num 2) (name CS) (type input))
        (pin (num 3) (name GND) (type input))
        (pin (num 4) (name OUT) (type input))
        (pin (num 5) (name OSC) (type input))))
    (libpart (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T)
      (description "Low Dropout Regulators")
      (docs https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) UZ1085L-ADJ-TA3-T))
      (pins
        (pin (num 1) (name A/G) (type input))
        (pin (num 2) (name OUT) (type input))
        (pin (num 3) (name IN) (type input))))
    (libpart (lib Switch) (part SW_DIP_x03)
      (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x3*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x03))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib Switch) (part SW_DPST_x2)
      (description "Single Pole Single Throw (SPST) switch, separate symbol")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DPST_x2))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name A) (type input))
        (pin (num 4) (name B) (type input)))))
  (libraries
    (library (logical Connector)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Connector.lib))
    (library (logical Device)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Device.lib))
    (library (logical Driver_LED)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Driver_LED.lib))
    (library (logical Regulator_Linear)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Regulator_Linear.lib))
    (library (logical Switch)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Switch.lib)))
  (nets
    (net (code 1) (name "Net-(R12-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref SW4) (pin 5)))
    (net (code 2) (name "Net-(R8-Pad1)")
      (node (ref SW4) (pin 4))
      (node (ref R8) (pin 1)))
    (net (code 3) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref SW4) (pin 6)))
    (net (code 4) (name GND)
      (node (ref RV2) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref RV2) (pin 3))
      (node (ref C2) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref RV7) (pin 2))
      (node (ref RV4) (pin 2))
      (node (ref RV4) (pin 3))
      (node (ref RV1) (pin 2))
      (node (ref RV1) (pin 3))
      (node (ref RV7) (pin 3))
      (node (ref C9) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref U6) (pin 3))
      (node (ref D3) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref J3) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref C15) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref U8) (pin 3))
      (node (ref C12) (pin 2))
      (node (ref U7) (pin 3)))
    (net (code 5) (name RawVoltage)
      (node (ref JP2) (pin 1))
      (node (ref SW5) (pin 2))
      (node (ref JP1) (pin 1))
      (node (ref JP3) (pin 1))
      (node (ref JP4) (pin 1)))
    (net (code 6) (name VDRIVER03)
      (node (ref JP8) (pin 1))
      (node (ref L3) (pin 2)))
    (net (code 7) (name VDRIVER04)
      (node (ref JP8) (pin 3))
      (node (ref L4) (pin 2)))
    (net (code 8) (name VDRIVER01)
      (node (ref JP7) (pin 1))
      (node (ref L1) (pin 2)))
    (net (code 9) (name LED01)
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref JP7) (pin 2)))
    (net (code 10) (name VDRIVER02)
      (node (ref JP7) (pin 3))
      (node (ref L2) (pin 2)))
    (net (code 11) (name "Net-(R12-Pad2)")
      (node (ref R7) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R12) (pin 2)))
    (net (code 12) (name "Net-(C16-Pad1)")
      (node (ref U8) (pin 5))
      (node (ref C16) (pin 1)))
    (net (code 13) (name "Net-(C15-Pad1)")
      (node (ref C15) (pin 1))
      (node (ref U7) (pin 5)))
    (net (code 14) (name "Net-(R6-Pad1)")
      (node (ref SW3) (pin 4))
      (node (ref R6) (pin 1)))
    (net (code 15) (name "Net-(R11-Pad1)")
      (node (ref SW3) (pin 5))
      (node (ref R11) (pin 1)))
    (net (code 16) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref SW3) (pin 6)))
    (net (code 17) (name "Net-(R11-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref U7) (pin 2)))
    (net (code 18) (name "Net-(D4-Pad1)")
      (node (ref L4) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref U8) (pin 4)))
    (net (code 19) (name "Net-(JP5-Pad3)")
      (node (ref RV1) (pin 1))
      (node (ref JP5) (pin 3)))
    (net (code 20) (name VPSU04)
      (node (ref SW4) (pin 3))
      (node (ref SW4) (pin 2))
      (node (ref SW4) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref RV8) (pin 2))
      (node (ref U8) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref RV8) (pin 1)))
    (net (code 21) (name "Net-(J4-Pad1)")
      (node (ref J4) (pin 1))
      (node (ref SW5) (pin 1)))
    (net (code 22) (name "Net-(C4-Pad1)")
      (node (ref JP4) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref C4) (pin 1)))
    (net (code 23) (name vari02)
      (node (ref RV6) (pin 3))
      (node (ref JP6) (pin 1))
      (node (ref RV7) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 24) (name LED02)
      (node (ref J3) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref JP8) (pin 2)))
    (net (code 25) (name "Net-(JP6-Pad3)")
      (node (ref RV2) (pin 1))
      (node (ref JP6) (pin 3)))
    (net (code 26) (name vari01)
      (node (ref RV4) (pin 1))
      (node (ref RV3) (pin 3))
      (node (ref JP5) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 27) (name "Net-(JP5-Pad2)")
      (node (ref JP5) (pin 2))
      (node (ref RV5) (pin 3))
      (node (ref U2) (pin 1)))
    (net (code 28) (name "Net-(JP6-Pad2)")
      (node (ref RV8) (pin 3))
      (node (ref JP6) (pin 2))
      (node (ref U4) (pin 1)))
    (net (code 29) (name "Net-(R1-Pad2)")
      (node (ref R9) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref R1) (pin 2)))
    (net (code 30) (name "Net-(C13-Pad1)")
      (node (ref U5) (pin 5))
      (node (ref C13) (pin 1)))
    (net (code 31) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref SW1) (pin 4)))
    (net (code 32) (name "Net-(R9-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref SW1) (pin 5)))
    (net (code 33) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref SW1) (pin 6)))
    (net (code 34) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref JP2) (pin 2)))
    (net (code 35) (name "Net-(C14-Pad1)")
      (node (ref C14) (pin 1))
      (node (ref U6) (pin 5)))
    (net (code 36) (name "Net-(D2-Pad1)")
      (node (ref U6) (pin 4))
      (node (ref D2) (pin 1))
      (node (ref L2) (pin 1)))
    (net (code 37) (name "Net-(R10-Pad2)")
      (node (ref R10) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref U6) (pin 2))
      (node (ref R3) (pin 2)))
    (net (code 38) (name "Net-(D1-Pad1)")
      (node (ref L1) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U5) (pin 4)))
    (net (code 39) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref JP1) (pin 2)))
    (net (code 40) (name VPSU01)
      (node (ref U5) (pin 1))
      (node (ref RV3) (pin 2))
      (node (ref RV3) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref SW1) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref SW1) (pin 3)))
    (net (code 41) (name "Net-(D3-Pad1)")
      (node (ref L3) (pin 1))
      (node (ref U7) (pin 4))
      (node (ref D3) (pin 1)))
    (net (code 42) (name "Net-(C3-Pad1)")
      (node (ref U3) (pin 3))
      (node (ref C3) (pin 1))
      (node (ref JP3) (pin 2)))
    (net (code 43) (name VPSU03)
      (node (ref RV6) (pin 2))
      (node (ref RV6) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref U7) (pin 1))
      (node (ref SW3) (pin 3))
      (node (ref SW3) (pin 2))
      (node (ref SW3) (pin 1))
      (node (ref C11) (pin 1)))
    (net (code 44) (name VPSU02)
      (node (ref U2) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref SW2) (pin 3))
      (node (ref RV5) (pin 2))
      (node (ref RV5) (pin 1)))
    (net (code 45) (name "Net-(R3-Pad1)")
      (node (ref SW2) (pin 6))
      (node (ref R3) (pin 1)))
    (net (code 46) (name "Net-(R10-Pad1)")
      (node (ref SW2) (pin 5))
      (node (ref R10) (pin 1)))
    (net (code 47) (name "Net-(R4-Pad1)")
      (node (ref SW2) (pin 4))
      (node (ref R4) (pin 1)))))