(export (version D)
  (design
    (source /home/hendrik/Schreibtisch/FilmLED/TestDriverV2/TestDriverV2.sch)
    (date "Fr 02 Aug 2019 21:49:46 CEST")
    (tool "Eeschema 5.1.2-5.1.2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title TestDriver)
        (company)
        (rev "Rev 2")
        (date 2019-08-02)
        (source TestDriverV2.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U9)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A1BC))
    (comp (ref C5)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A4B2))
    (comp (ref R5)
      (value "Dummy Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A521))
    (comp (ref D1)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A689))
    (comp (ref L1)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7A6E3))
    (comp (ref C1)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7EB69))
    (comp (ref C3)
      (value "47 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA7EC87))
    (comp (ref U3)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C70CFFF))
    (comp (ref U4)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C70D081))
    (comp (ref U5)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C70D12B))
    (comp (ref U13)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C726DB0))
    (comp (ref C9)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C726DBC))
    (comp (ref D5)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C726DC8))
    (comp (ref L5)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C726DCE))
    (comp (ref C2)
      (value "22 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72DE5D))
    (comp (ref C4)
      (value "47 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72DE63))
    (comp (ref U6)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72DE77))
    (comp (ref U7)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72DE7D))
    (comp (ref U8)
      (value UZ1085L-ADJ-TA3-T)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (libsource (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T) (description "Low Dropout Regulators"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72DE83))
    (comp (ref R1)
      (value "255 KΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B7A63))
    (comp (ref R2)
      (value "255 KΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C72E0CB))
    (comp (ref Q1)
      (value UP2855G-AA3-R)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BCE) (description "Transistor PNP (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C73DA08))
    (comp (ref R3)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C75C23D))
    (comp (ref Q2)
      (value UP2855G-AA3-R)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BCE) (description "Transistor PNP (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C78AA1E))
    (comp (ref R4)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C78AA29))
    (comp (ref J1)
      (value Conn_01x03_Male)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x03_Male) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C835A45))
    (comp (ref J2)
      (value Conn_01x02_Male)
      (footprint Connector_Wire:SolderWirePad_1x02_P5.08mm_Drill1.5mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C879272))
    (comp (ref J4)
      (value Conn_01x02_Male)
      (footprint own:SolderPad_2_Pin)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8D5A15))
    (comp (ref J5)
      (value Conn_01x02_Male)
      (footprint own:SolderPad_2_Pin)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9046D8))
    (comp (ref J3)
      (value Conn_01x10_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x10_Male) (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA277EF))
    (comp (ref R6)
      (value "Dummy Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBADBAE))
    (comp (ref U10)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD1E2))
    (comp (ref C6)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD1E8))
    (comp (ref D2)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD1EE))
    (comp (ref L2)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD1F4))
    (comp (ref U14)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD212))
    (comp (ref C10)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD218))
    (comp (ref D6)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD21E))
    (comp (ref L6)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBD224))
    (comp (ref U11)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7862))
    (comp (ref C7)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7868))
    (comp (ref D3)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC786E))
    (comp (ref L3)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7874))
    (comp (ref U15)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7892))
    (comp (ref C11)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7898))
    (comp (ref D7)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC789E))
    (comp (ref L7)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC78A4))
    (comp (ref U12)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC78CA))
    (comp (ref C8)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC78D0))
    (comp (ref D4)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC78D6))
    (comp (ref L4)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC78DC))
    (comp (ref U16)
      (value AMC7150)
      (footprint Package_TO_SOT_SMD:TO-252-5_TabPin3)
      (datasheet https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (libsource (lib Driver_LED) (part AMC7150) (description "1.5A POWER LED DRIVER"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC78FA))
    (comp (ref C12)
      (value "750 pF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7900))
    (comp (ref D8)
      (value D_Schottky)
      (footprint Diode_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC7906))
    (comp (ref L8)
      (value "220 µH")
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC790C))
    (comp (ref U1)
      (value CAT5140)
      (footprint Package_SO:MSOP-8_3x3mm_P0.65mm)
      (datasheet http://static6.arrow.com/aropdfconversion/908174aa20c602eaac91f194663e9d5657052dee/765cat5140-d.pdf)
      (libsource (lib Potentiometer_Digital) (part CAT5140) (description "Single Channel 256 Tap Digital Potentiometer (POT)with Integrated EEPROMand I2C Control"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D48768C))
    (comp (ref U2)
      (value CAT5140)
      (footprint Package_SO:MSOP-8_3x3mm_P0.65mm)
      (datasheet http://static6.arrow.com/aropdfconversion/908174aa20c602eaac91f194663e9d5657052dee/765cat5140-d.pdf)
      (libsource (lib Potentiometer_Digital) (part CAT5140) (description "Single Channel 256 Tap Digital Potentiometer (POT)with Integrated EEPROMand I2C Control"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4884C6)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector) (part Conn_01x10_Male)
      (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x10_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Q_PNP_BCE)
      (description "Transistor PNP (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PNP_BCE))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name C) (type passive))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Driver_LED) (part AMC7150)
      (description "1.5A POWER LED DRIVER")
      (docs https://datasheet.lcsc.com/szlcsc/ADDtek-Corp-AMC7150_C18354.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) AMC7150))
      (pins
        (pin (num 1) (name VCC) (type input))
        (pin (num 2) (name CS) (type input))
        (pin (num 3) (name GND) (type input))
        (pin (num 4) (name OUT) (type input))
        (pin (num 5) (name OSC) (type input))))
    (libpart (lib Potentiometer_Digital) (part CAT5140)
      (description "Single Channel 256 Tap Digital Potentiometer (POT)with Integrated EEPROMand I2C Control")
      (docs http://static6.arrow.com/aropdfconversion/908174aa20c602eaac91f194663e9d5657052dee/765cat5140-d.pdf)
      (footprints
        (fp MSOP_8))
      (fields
        (field (name Reference) U)
        (field (name Value) CAT5140))
      (pins
        (pin (num 1) (name ~WP) (type input))
        (pin (num 2) (name SCL) (type input))
        (pin (num 3) (name SDA) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name RW) (type BiDi))
        (pin (num 6) (name RL) (type BiDi))
        (pin (num 7) (name RH) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Regulator_Linear) (part UZ1085L-ADJ-TA3-T)
      (description "Low Dropout Regulators")
      (docs https://datasheet.lcsc.com/szlcsc/Unisonic-Tech-UZ1085L-ADJ-TA3-T_C95078.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) UZ1085L-ADJ-TA3-T))
      (pins
        (pin (num 1) (name A/G) (type input))
        (pin (num 2) (name OUT) (type input))
        (pin (num 3) (name IN) (type input)))))
  (libraries
    (library (logical Connector)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Connector.lib))
    (library (logical Device)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Device.lib))
    (library (logical Driver_LED)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Driver_LED.lib))
    (library (logical Potentiometer_Digital)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Potentiometer_Digital.lib))
    (library (logical Regulator_Linear)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Regulator_Linear.lib)))
  (nets
    (net (code 1) (name "Net-(C10-Pad1)")
      (node (ref U14) (pin 5))
      (node (ref C10) (pin 1)))
    (net (code 2) (name "Net-(C6-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref U10) (pin 5)))
    (net (code 3) (name "Net-(D6-Pad1)")
      (node (ref L6) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref U14) (pin 4)))
    (net (code 4) (name GND)
      (node (ref D1) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U9) (pin 3))
      (node (ref U1) (pin 4))
      (node (ref J1) (pin 3))
      (node (ref U10) (pin 3))
      (node (ref C6) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref U16) (pin 3))
      (node (ref C12) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U13) (pin 3))
      (node (ref C9) (pin 2))
      (node (ref U12) (pin 3))
      (node (ref D4) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref U15) (pin 3))
      (node (ref C11) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref J3) (pin 10))
      (node (ref R1) (pin 1))
      (node (ref U14) (pin 3))
      (node (ref D6) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref U11) (pin 3))
      (node (ref R2) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref J4) (pin 2)))
    (net (code 5) (name VPSU02)
      (node (ref U2) (pin 7))
      (node (ref R6) (pin 1))
      (node (ref U15) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U6) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref U7) (pin 2))
      (node (ref U13) (pin 1))
      (node (ref U14) (pin 1))
      (node (ref U16) (pin 1)))
    (net (code 6) (name VDRIVER02)
      (node (ref L6) (pin 2))
      (node (ref L5) (pin 2))
      (node (ref L7) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref L8) (pin 2)))
    (net (code 7) (name VDRIVER01)
      (node (ref L2) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref L3) (pin 2))
      (node (ref L4) (pin 2))
      (node (ref L1) (pin 2)))
    (net (code 8) (name "Net-(D2-Pad1)")
      (node (ref U10) (pin 4))
      (node (ref L2) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 9) (name VPSU01)
      (node (ref U12) (pin 1))
      (node (ref U9) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref U1) (pin 7))
      (node (ref C3) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U11) (pin 1))
      (node (ref U10) (pin 1)))
    (net (code 10) (name Iset02)
      (node (ref U13) (pin 2))
      (node (ref U15) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U14) (pin 2))
      (node (ref U16) (pin 2)))
    (net (code 11) (name "Net-(C7-Pad1)")
      (node (ref C7) (pin 1))
      (node (ref U11) (pin 5)))
    (net (code 12) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref L3) (pin 1))
      (node (ref U11) (pin 4)))
    (net (code 13) (name Iset01)
      (node (ref U11) (pin 2))
      (node (ref U10) (pin 2))
      (node (ref U9) (pin 2))
      (node (ref U12) (pin 2))
      (node (ref R5) (pin 2)))
    (net (code 14) (name Q02)
      (node (ref R4) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 15) (name SCL01)
      (node (ref U1) (pin 2))
      (node (ref J3) (pin 3)))
    (net (code 16) (name SDA01)
      (node (ref J3) (pin 4))
      (node (ref U1) (pin 3)))
    (net (code 17) (name temp01)
      (node (ref J3) (pin 7))
      (node (ref J4) (pin 1)))
    (net (code 18) (name temp02)
      (node (ref J5) (pin 1))
      (node (ref J3) (pin 8)))
    (net (code 19) (name "Net-(C12-Pad1)")
      (node (ref C12) (pin 1))
      (node (ref U16) (pin 5)))
    (net (code 20) (name "Net-(D8-Pad1)")
      (node (ref L8) (pin 1))
      (node (ref D8) (pin 1))
      (node (ref U16) (pin 4)))
    (net (code 21) (name "Net-(D4-Pad1)")
      (node (ref U12) (pin 4))
      (node (ref L4) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 22) (name "Net-(C8-Pad1)")
      (node (ref C8) (pin 1))
      (node (ref U12) (pin 5)))
    (net (code 23) (name SDA02)
      (node (ref U2) (pin 3))
      (node (ref J3) (pin 6)))
    (net (code 24) (name +5V)
      (node (ref J3) (pin 9))
      (node (ref U1) (pin 8))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 25) (name "Net-(C11-Pad1)")
      (node (ref U15) (pin 5))
      (node (ref C11) (pin 1)))
    (net (code 26) (name "Net-(D7-Pad1)")
      (node (ref U15) (pin 4))
      (node (ref D7) (pin 1))
      (node (ref L7) (pin 1)))
    (net (code 27) (name "Net-(D5-Pad1)")
      (node (ref U13) (pin 4))
      (node (ref D5) (pin 1))
      (node (ref L5) (pin 1)))
    (net (code 28) (name ADJ01)
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 6))
      (node (ref R1) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 29) (name "Net-(C9-Pad1)")
      (node (ref U13) (pin 5))
      (node (ref C9) (pin 1)))
    (net (code 30) (name RawVoltage)
      (node (ref U5) (pin 3))
      (node (ref U3) (pin 3))
      (node (ref U4) (pin 3))
      (node (ref U8) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref U6) (pin 3))
      (node (ref C2) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref U7) (pin 3)))
    (net (code 31) (name "Net-(D1-Pad1)")
      (node (ref L1) (pin 1))
      (node (ref U9) (pin 4))
      (node (ref D1) (pin 1)))
    (net (code 32) (name "Net-(C5-Pad1)")
      (node (ref U9) (pin 5))
      (node (ref C5) (pin 1)))
    (net (code 33) (name LED01)
      (node (ref Q1) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 34) (name "Net-(Q1-Pad1)")
      (node (ref R3) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 35) (name Q01)
      (node (ref J3) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 36) (name SCL02)
      (node (ref U2) (pin 2))
      (node (ref J3) (pin 5)))
    (net (code 37) (name "Net-(Q2-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 38) (name LED02)
      (node (ref J1) (pin 1))
      (node (ref Q2) (pin 2)))
    (net (code 39) (name ADJ02)
      (node (ref U8) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref U2) (pin 5))
      (node (ref R2) (pin 2)))))