(export (version D)
  (design
    (source /home/hendrik/Schreibtisch/OpenChargeMicro/Platine/OpenChargeMicro/OpenChargeMicro.sch)
    (date "Sa 22 Sep 2018 21:03:55 CEST")
    (tool "Eeschema 5.0.0")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title OpenChargeMicro)
        (company CopterSicht)
        (rev "Rev 1")
        (date 2018-09-16)
        (source OpenChargeMicro.sch)
        (comment (number 1) (value "GPL 3.0"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref SW1)
      (value cS01)
      (footprint Button_Switch_THT:SW_DIP_SPSTx05_Slide_9.78x14.88mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x05) (description "5x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E0E33))
    (comp (ref R21)
      (value "30 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E102E))
    (comp (ref R33)
      (value "20 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E1087))
    (comp (ref R22)
      (value "5 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E10DA))
    (comp (ref R34)
      (value "3 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E112C))
    (comp (ref R23)
      (value "1k66 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E11B4))
    (comp (ref J6)
      (value Bat01_MX)
      (footprint Connector_Molex:Molex_PicoBlade_53047-0410_1x02_P1.25mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E2934))
    (comp (ref J4)
      (value USB_B_Mini)
      (footprint Connector_USB:USB_Mini-B_Lumberg_2486_01_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Mini) (description "USB Mini Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E3B00))
    (comp (ref D1)
      (value cLED01)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E5826))
    (comp (ref D2)
      (value sLED01)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E58F0))
    (comp (ref R47)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E599D))
    (comp (ref R48)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9E5AF8))
    (comp (ref U6)
      (value TP4056)
      (footprint Package_SO:SOP-8_EP_150mil)
      (datasheet https://datasheet.lcsc.com/szlcsc/Nanjing-Extension-Microelectronics-TP4056_C16581.pdf)
      (libsource (lib Battery_Management) (part TP4056) (description "PMIC - Battery Management"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6D97))
    (comp (ref SW2)
      (value cS02)
      (footprint Button_Switch_THT:SW_DIP_SPSTx05_Slide_9.78x14.88mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x05) (description "5x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6D9D))
    (comp (ref R24)
      (value "30 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6DA3))
    (comp (ref R35)
      (value "20 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6DA9))
    (comp (ref R25)
      (value "5 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6DAF))
    (comp (ref R36)
      (value "3 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6DB5))
    (comp (ref R26)
      (value "1k66 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6DBB))
    (comp (ref J7)
      (value Bat02_Molex)
      (footprint Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6DEF))
    (comp (ref D3)
      (value cLED02)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6E08))
    (comp (ref D4)
      (value sLED02)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6E0E))
    (comp (ref R49)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6E14))
    (comp (ref R50)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F6E1A))
    (comp (ref U7)
      (value TP4056)
      (footprint Package_SO:SOP-8_EP_150mil)
      (datasheet https://datasheet.lcsc.com/szlcsc/Nanjing-Extension-Microelectronics-TP4056_C16581.pdf)
      (libsource (lib Battery_Management) (part TP4056) (description "PMIC - Battery Management"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F9488))
    (comp (ref SW3)
      (value cS03)
      (footprint Button_Switch_THT:SW_DIP_SPSTx05_Slide_9.78x14.88mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x05) (description "5x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F948E))
    (comp (ref R27)
      (value "30 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F9494))
    (comp (ref R37)
      (value "20 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F949A))
    (comp (ref R28)
      (value "5 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F94A0))
    (comp (ref R38)
      (value "3 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F94A6))
    (comp (ref R29)
      (value "1k66 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F94AC))
    (comp (ref J8)
      (value Bat03_Molex)
      (footprint Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F94E0))
    (comp (ref D5)
      (value cLED03)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F94F9))
    (comp (ref D6)
      (value sLED03)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F94FF))
    (comp (ref R51)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F9505))
    (comp (ref R52)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9F950B))
    (comp (ref U8)
      (value TP4056)
      (footprint Package_SO:SOP-8_EP_150mil)
      (datasheet https://datasheet.lcsc.com/szlcsc/Nanjing-Extension-Microelectronics-TP4056_C16581.pdf)
      (libsource (lib Battery_Management) (part TP4056) (description "PMIC - Battery Management"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE898))
    (comp (ref SW4)
      (value cS04)
      (footprint Button_Switch_THT:SW_DIP_SPSTx05_Slide_9.78x14.88mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x05) (description "5x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE89E))
    (comp (ref R30)
      (value "30 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE8A4))
    (comp (ref R39)
      (value "20 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE8AA))
    (comp (ref R31)
      (value "5 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE8B0))
    (comp (ref R40)
      (value "3 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE8B6))
    (comp (ref R32)
      (value "1k66 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE8BC))
    (comp (ref J9)
      (value Bat04_Molex)
      (footprint Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE8F0))
    (comp (ref D7)
      (value cLED04)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE909))
    (comp (ref D8)
      (value sLED04)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE90F))
    (comp (ref R53)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE915))
    (comp (ref R54)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FE91B))
    (comp (ref R11)
      (value "560 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA086E5))
    (comp (ref R15)
      (value "2 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA0890E))
    (comp (ref R12)
      (value "560 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA4C5B0))
    (comp (ref R16)
      (value "2 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA4C5B6))
    (comp (ref R13)
      (value "560 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA57816))
    (comp (ref R17)
      (value "2 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA5781C))
    (comp (ref R14)
      (value "560 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA6398F))
    (comp (ref R18)
      (value "2 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA63995))
    (comp (ref J2)
      (value "128X64 OLED")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAD0625))
    (comp (ref R46)
      (value "0.01 Ω")
      (footprint Resistor_SMD:R_Shunt_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FBCF3))
    (comp (ref U2)
      (value LM324DR)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet https://datasheet.lcsc.com/szlcsc/Texas-Instruments-TI-LM324DR_C7943.pdf)
      (libsource (lib Amplifier_Operational) (part LM324DR) (description "General Purpose Amplifiers"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FD6E8))
    (comp (ref U4)
      (value CD4051BM96)
      (footprint Package_SO:SOIC-16_3.9x9.9mm_P1.27mm)
      (datasheet https://datasheet.lcsc.com/szlcsc/Texas-Instruments-TI-CD4051BM96_C21379.pdf)
      (libsource (lib 4xxx) (part CD4051BM96) (description "4000 Series Multiplexer/Demultiplexer"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9FEF61))
    (comp (ref R43)
      (value "0.01 Ω")
      (footprint Resistor_SMD:R_Shunt_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC991FF))
    (comp (ref R44)
      (value "0.01 Ω")
      (footprint Resistor_SMD:R_Shunt_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC993D3))
    (comp (ref R45)
      (value "0.01 Ω")
      (footprint Resistor_SMD:R_Shunt_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC99493))
    (comp (ref R1)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BDB1854))
    (comp (ref R3)
      (value "1 MΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BDB1BEC))
    (comp (ref R4)
      (value "1 MΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BE3FFD8))
    (comp (ref R2)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BE40088))
    (comp (ref R5)
      (value "1 MΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF2C36C))
    (comp (ref R7)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF2CB32))
    (comp (ref R6)
      (value "1 MΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFD7F12))
    (comp (ref R8)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFD7FC6))
    (comp (ref J3)
      (value "Power Input")
      (footprint Connector_BarrelJack:BarrelJack_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1D7BB3))
    (comp (ref U1)
      (value AMS1084CM-5.0)
      (footprint Package_TO_SOT_SMD:TO-263-3_TabPin2)
      (datasheet http://www.advanced-monolithic.com/pdf/ds1117.pdf)
      (libsource (lib Regulator_Linear) (part AMS1117-5.0) (description "1A Low Dropout regulator, positive, 5.0V fixed output, SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1D81BE))
    (comp (ref C1)
      (value "10 µF")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-2012-12_Kemet-R)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C23FC45))
    (comp (ref C2)
      (value "100 nF")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C23FDBC))
    (comp (ref R19)
      (value "560 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3196FC))
    (comp (ref R20)
      (value "2 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C319702))
    (comp (ref R41)
      (value "1k7 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3B621B))
    (comp (ref R42)
      (value "800 Ω")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3B6221))
    (comp (ref Q2)
      (value UP2855G-AA3-R)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BCE) (description "Transistor PNP (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C483696))
    (comp (ref R10)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C483E2D))
    (comp (ref U5)
      (value TP4056)
      (footprint Package_SO:SOP-8_EP_150mil)
      (datasheet https://datasheet.lcsc.com/szlcsc/Nanjing-Extension-Microelectronics-TP4056_C16581.pdf)
      (libsource (lib Battery_Management) (part TP4056) (description "PMIC - Battery Management"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9D890A))
    (comp (ref Q1)
      (value 2N3906)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (libsource (lib Transistor_BJT) (part 2N3906) (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B7D1F))
    (comp (ref R9)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B7FEF))
    (comp (ref BZ1)
      (value Buzzer)
      (footprint Buzzer_Beeper:Buzzer_12x9.5RM7.6)
      (datasheet ~)
      (libsource (lib Device) (part Buzzer) (description "Buzzer, polar"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B829B))
    (comp (ref J1)
      (value "Bluethooth HM-10")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06_Male) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9F6EC3))
    (comp (ref J5)
      (value "Serial Port")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x05_Male) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBD8AF4))
    (comp (ref J10)
      (value Bat01_Molex)
      (footprint Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA33106))
    (comp (ref J11)
      (value Bat01_mCPX)
      (footprint Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA33269))
    (comp (ref J12)
      (value Bat02_mCPX)
      (footprint Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC3873F))
    (comp (ref J13)
      (value Bat02_MX)
      (footprint Connector_Molex:Molex_PicoBlade_53047-0410_1x02_P1.25mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC3880D))
    (comp (ref J16)
      (value Bat03_mCPX)
      (footprint Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BDCBE8A))
    (comp (ref J17)
      (value Bat03_MX)
      (footprint Connector_Molex:Molex_PicoBlade_53047-0410_1x02_P1.25mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BDCBF60))
    (comp (ref J14)
      (value Bat04_mCPX)
      (footprint Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF05582))
    (comp (ref J15)
      (value Bat04_MX)
      (footprint Connector_Molex:Molex_PicoBlade_53047-0410_1x02_P1.25mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF05658))
    (comp (ref U3)
      (value DevBoardV3)
      (footprint own:DevBoardV3)
      (libsource (lib DevBoard) (part DevBoardV3) (description "DevBoard V3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9D71A9)))
  (libparts
    (libpart (lib 4xxx) (part CD4051BM96)
      (description "4000 Series Multiplexer/Demultiplexer")
      (docs https://datasheet.lcsc.com/szlcsc/Texas-Instruments-TI-CD4051BM96_C21379.pdf)
      (footprints
        (fp SOIC-16_150mil))
      (fields
        (field (name Reference) U)
        (field (name Value) CD4051BM96))
      (pins
        (pin (num 1) (name y4) (type BiDi))
        (pin (num 2) (name y6) (type BiDi))
        (pin (num 3) (name z) (type BiDi))
        (pin (num 4) (name y7) (type BiDi))
        (pin (num 5) (name y5) (type BiDi))
        (pin (num 6) (name E) (type input))
        (pin (num 7) (name Vee) (type input))
        (pin (num 8) (name GND) (type input))
        (pin (num 9) (name S2) (type input))
        (pin (num 10) (name S1) (type input))
        (pin (num 11) (name S0) (type input))
        (pin (num 12) (name y3) (type BiDi))
        (pin (num 13) (name y0) (type BiDi))
        (pin (num 14) (name y1) (type BiDi))
        (pin (num 15) (name y2) (type BiDi))
        (pin (num 16) (name Vcc) (type input))))
    (libpart (lib Amplifier_Operational) (part LM324DR)
      (description "General Purpose Amplifiers")
      (docs https://datasheet.lcsc.com/szlcsc/Texas-Instruments-TI-LM324DR_C7943.pdf)
      (footprints
        (fp SOIC-14_150mil))
      (fields
        (field (name Reference) U)
        (field (name Value) LM324DR))
      (pins
        (pin (num 1) (name 1OUT) (type output))
        (pin (num 2) (name 1IN-) (type input))
        (pin (num 3) (name 1IN+) (type input))
        (pin (num 4) (name Vcc) (type input))
        (pin (num 5) (name 2IN+) (type input))
        (pin (num 6) (name 2IN-) (type input))
        (pin (num 7) (name 2OUT) (type output))
        (pin (num 8) (name 3OUT) (type output))
        (pin (num 9) (name 3IN-) (type input))
        (pin (num 10) (name 3IN+) (type input))
        (pin (num 11) (name GND) (type input))
        (pin (num 12) (name 4IN+) (type input))
        (pin (num 13) (name 4IN-) (type input))
        (pin (num 14) (name 4OUT) (type output))))
    (libpart (lib Battery_Management) (part TP4056)
      (description "PMIC - Battery Management")
      (docs https://datasheet.lcsc.com/szlcsc/Nanjing-Extension-Microelectronics-TP4056_C16581.pdf)
      (footprints
        (fp SOP-8_EP_150mil))
      (fields
        (field (name Reference) U)
        (field (name Value) TP4056))
      (pins
        (pin (num 1) (name TEMP) (type input))
        (pin (num 2) (name PROG) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name Vcc) (type power_in))
        (pin (num 5) (name BAT) (type power_out))
        (pin (num 6) (name STDBY) (type output))
        (pin (num 7) (name CHRG) (type output))
        (pin (num 8) (name CE) (type BiDi))))
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x04_Male)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector) (part Conn_01x05_Male)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Connector) (part Conn_01x06_Male)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib DevBoard) (part DevBoardV3)
      (description "DevBoard V3")
      (fields
        (field (name Reference) U)
        (field (name Value) DevBoardV3))
      (pins
        (pin (num 1) (name GND) (type power_out))
        (pin (num 2) (name D5) (type BiDi))
        (pin (num 3) (name D6) (type BiDi))
        (pin (num 4) (name D7) (type BiDi))
        (pin (num 5) (name D8) (type BiDi))
        (pin (num 6) (name D9) (type BiDi))
        (pin (num 7) (name D10) (type BiDi))
        (pin (num 8) (name D11/MOSI) (type BiDi))
        (pin (num 9) (name D12/MISO) (type BiDi))
        (pin (num 10) (name D13/SCK) (type BiDi))
        (pin (num 11) (name T01) (type output))
        (pin (num 12) (name T02) (type output))
        (pin (num 13) (name Vin) (type power_in))
        (pin (num 14) (name GND) (type power_out))
        (pin (num 15) (name A0) (type power_out))
        (pin (num 16) (name A1) (type output))
        (pin (num 17) (name A2) (type input))
        (pin (num 18) (name A3) (type input))
        (pin (num 19) (name A4) (type output))
        (pin (num 20) (name A5) (type BiDi))
        (pin (num 21) (name WS2812B) (type BiDi))
        (pin (num 22) (name RST) (type BiDi))
        (pin (num 23) (name Rx) (type BiDi))
        (pin (num 24) (name Tx) (type BiDi))
        (pin (num 25) (name 3V3) (type BiDi))
        (pin (num 26) (name 5V) (type power_out))))
    (libpart (lib Device) (part Buzzer)
      (description "Buzzer, polar")
      (docs ~)
      (footprints
        (fp *Buzzer*))
      (fields
        (field (name Reference) BZ)
        (field (name Value) Buzzer))
      (pins
        (pin (num 1) (name -) (type passive))
        (pin (num 2) (name +) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part LED)
      (description "LED generic")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Q_PNP_BCE)
      (description "Transistor PNP (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PNP_BCE))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name C) (type passive))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Shunt)
      (description "Shunt Resistor")
      (docs ~)
      (footprints
        (fp R_*Shunt*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Shunt))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Regulator_Linear) (part AP1117-15)
      (aliases
        (alias AP1117-18)
        (alias AP1117-25)
        (alias AP1117-33)
        (alias AP1117-50)
        (alias LD1117S33TR_SOT223)
        (alias LD1117S12TR_SOT223)
        (alias LD1117S18TR_SOT223)
        (alias LD1117S25TR_SOT223)
        (alias LD1117S50TR_SOT223)
        (alias NCP1117-12_SOT223)
        (alias NCP1117-1.5_SOT223)
        (alias NCP1117-1.8_SOT223)
        (alias NCP1117-2.0_SOT223)
        (alias NCP1117-2.5_SOT223)
        (alias NCP1117-2.85_SOT223)
        (alias NCP1117-3.3_SOT223)
        (alias NCP1117-5.0_SOT223)
        (alias AMS1117-1.5)
        (alias AMS1117-1.8)
        (alias AMS1117-2.5)
        (alias AMS1117-2.85)
        (alias AMS1117-3.3)
        (alias AMS1117-5.0))
      (description "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT?223*TabPin2*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117-15)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-223-3_TabPin2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Switch) (part SW_DIP_x05)
      (description "5x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x5*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x05))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))))
    (libpart (lib Transistor_BJT) (part 2N3906)
      (aliases
        (alias 2N3905))
      (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3906)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive)))))
  (libraries
    (library (logical 4xxx)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/4xxx.lib))
    (library (logical Amplifier_Operational)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Amplifier_Operational.lib))
    (library (logical Battery_Management)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Battery_Management.lib))
    (library (logical Connector)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Connector.lib))
    (library (logical DevBoard)
      (uri /home/hendrik/Schreibtisch/OpenRClight/Platine/OpenRClight/DevBoard.lib))
    (library (logical Device)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Device.lib))
    (library (logical Regulator_Linear)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Regulator_Linear.lib))
    (library (logical Switch)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Switch.lib))
    (library (logical Transistor_BJT)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Transistor_BJT.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref J4) (pin 5))
      (node (ref U6) (pin 3))
      (node (ref R15) (pin 1))
      (node (ref R45) (pin 4))
      (node (ref SW2) (pin 5))
      (node (ref R45) (pin 3))
      (node (ref R44) (pin 4))
      (node (ref R44) (pin 3))
      (node (ref R43) (pin 4))
      (node (ref R7) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref R18) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref SW3) (pin 3))
      (node (ref R17) (pin 1))
      (node (ref SW3) (pin 1))
      (node (ref SW3) (pin 2))
      (node (ref R43) (pin 3))
      (node (ref SW3) (pin 4))
      (node (ref SW3) (pin 5))
      (node (ref R16) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref BZ1) (pin 2))
      (node (ref R46) (pin 4))
      (node (ref R46) (pin 3))
      (node (ref J3) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref SW1) (pin 5))
      (node (ref SW1) (pin 4))
      (node (ref SW1) (pin 3))
      (node (ref SW1) (pin 2))
      (node (ref U2) (pin 11))
      (node (ref SW4) (pin 5))
      (node (ref C1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref J5) (pin 5))
      (node (ref U3) (pin 14))
      (node (ref J1) (pin 3))
      (node (ref R8) (pin 2))
      (node (ref SW2) (pin 3))
      (node (ref U4) (pin 6))
      (node (ref R42) (pin 1))
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 8))
      (node (ref SW2) (pin 4))
      (node (ref U5) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref SW4) (pin 2))
      (node (ref SW4) (pin 4))
      (node (ref SW4) (pin 1))
      (node (ref U8) (pin 3))
      (node (ref U8) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref U7) (pin 3))
      (node (ref SW4) (pin 3)))
    (net (code 2) (name +5V)
      (node (ref J4) (pin 1))
      (node (ref U3) (pin 13))
      (node (ref Q1) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref U3) (pin 26))
      (node (ref J5) (pin 1))
      (node (ref U4) (pin 16))
      (node (ref Q2) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R19) (pin 1)))
    (net (code 3) (name Ain08)
      (node (ref U2) (pin 14))
      (node (ref U4) (pin 4))
      (node (ref R5) (pin 2)))
    (net (code 4) (name "Net-(R6-Pad1)")
      (node (ref U2) (pin 9))
      (node (ref R6) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 5) (name Ain07)
      (node (ref U4) (pin 2))
      (node (ref U2) (pin 8))
      (node (ref R6) (pin 2)))
    (net (code 6) (name Charge5V)
      (node (ref R53) (pin 1))
      (node (ref U7) (pin 4))
      (node (ref Q2) (pin 2))
      (node (ref U6) (pin 4))
      (node (ref R52) (pin 1))
      (node (ref R54) (pin 1))
      (node (ref R51) (pin 1))
      (node (ref U5) (pin 8))
      (node (ref U6) (pin 8))
      (node (ref U7) (pin 8))
      (node (ref R50) (pin 1))
      (node (ref U8) (pin 4))
      (node (ref R49) (pin 1))
      (node (ref U8) (pin 8))
      (node (ref R47) (pin 1))
      (node (ref U5) (pin 4))
      (node (ref R48) (pin 1)))
    (net (code 7) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R10) (pin 1)))
    (net (code 8) (name 15V_Probe)
      (node (ref R42) (pin 2))
      (node (ref R41) (pin 2))
      (node (ref U3) (pin 16)))
    (net (code 9) (name PowerOn)
      (node (ref U3) (pin 5))
      (node (ref R10) (pin 2)))
    (net (code 10) (name "Net-(D2-Pad1)")
      (node (ref U5) (pin 6))
      (node (ref D2) (pin 1)))
    (net (code 11) (name "Net-(D1-Pad1)")
      (node (ref U5) (pin 7))
      (node (ref D1) (pin 1)))
    (net (code 12) (name 5V_Probe)
      (node (ref R19) (pin 2))
      (node (ref U3) (pin 17))
      (node (ref R20) (pin 2)))
    (net (code 13) (name 15V)
      (node (ref U1) (pin 3))
      (node (ref J3) (pin 1))
      (node (ref R41) (pin 1)))
    (net (code 14) (name Current01)
      (node (ref R46) (pin 2))
      (node (ref U2) (pin 3)))
    (net (code 15) (name "Net-(J14-Pad1)")
      (node (ref J9) (pin 1))
      (node (ref J14) (pin 1))
      (node (ref J15) (pin 1))
      (node (ref R45) (pin 1)))
    (net (code 16) (name Current02)
      (node (ref U2) (pin 5))
      (node (ref R43) (pin 2)))
    (net (code 17) (name Current03)
      (node (ref U2) (pin 10))
      (node (ref R44) (pin 2)))
    (net (code 18) (name S0)
      (node (ref U3) (pin 2))
      (node (ref U4) (pin 11)))
    (net (code 19) (name S1)
      (node (ref U3) (pin 3))
      (node (ref U4) (pin 10)))
    (net (code 20) (name S2)
      (node (ref U4) (pin 9))
      (node (ref U3) (pin 4)))
    (net (code 21) (name "Net-(R2-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref U2) (pin 6)))
    (net (code 22) (name Ain06)
      (node (ref U4) (pin 5))
      (node (ref R4) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 23) (name "Net-(R5-Pad1)")
      (node (ref U2) (pin 13))
      (node (ref R7) (pin 1))
      (node (ref R5) (pin 1)))
    (net (code 24) (name Current04)
      (node (ref R45) (pin 2))
      (node (ref U2) (pin 12)))
    (net (code 25) (name "Net-(R1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 26) (name Ain05)
      (node (ref U2) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 27) (name "Net-(J16-Pad1)")
      (node (ref J17) (pin 1))
      (node (ref J8) (pin 1))
      (node (ref R44) (pin 1))
      (node (ref J16) (pin 1)))
    (net (code 28) (name "Net-(J12-Pad1)")
      (node (ref R43) (pin 1))
      (node (ref J13) (pin 1))
      (node (ref J7) (pin 1))
      (node (ref J12) (pin 1)))
    (net (code 29) (name Rx)
      (node (ref J5) (pin 4))
      (node (ref U3) (pin 23)))
    (net (code 30) (name "Net-(U3-Pad9)")
      (node (ref U3) (pin 9)))
    (net (code 31) (name +3V3)
      (node (ref J1) (pin 2))
      (node (ref U3) (pin 25))
      (node (ref J5) (pin 2)))
    (net (code 32) (name Tx)
      (node (ref U3) (pin 24))
      (node (ref J5) (pin 3)))
    (net (code 33) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 34) (name "Net-(U3-Pad21)")
      (node (ref U3) (pin 21)))
    (net (code 35) (name "Net-(U3-Pad22)")
      (node (ref U3) (pin 22)))
    (net (code 36) (name "Net-(U3-Pad10)")
      (node (ref U3) (pin 10)))
    (net (code 37) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11)))
    (net (code 38) (name "Net-(U3-Pad12)")
      (node (ref U3) (pin 12)))
    (net (code 39) (name "Net-(Q1-Pad2)")
      (node (ref R9) (pin 1))
      (node (ref Q1) (pin 2)))
    (net (code 40) (name "Net-(BZ1-Pad1)")
      (node (ref BZ1) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 41) (name Buzzer)
      (node (ref R9) (pin 2))
      (node (ref U3) (pin 6)))
    (net (code 42) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 43) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 44) (name "Net-(J10-Pad1)")
      (node (ref J11) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref R46) (pin 1))
      (node (ref J6) (pin 1)))
    (net (code 45) (name vTx)
      (node (ref J1) (pin 5))
      (node (ref U3) (pin 8)))
    (net (code 46) (name vRx)
      (node (ref U3) (pin 7))
      (node (ref J1) (pin 4)))
    (net (code 47) (name "Net-(D4-Pad1)")
      (node (ref U6) (pin 6))
      (node (ref D4) (pin 1)))
    (net (code 48) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref R49) (pin 2)))
    (net (code 49) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref R50) (pin 2)))
    (net (code 50) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref U6) (pin 7)))
    (net (code 51) (name "Net-(D6-Pad1)")
      (node (ref U7) (pin 6))
      (node (ref D6) (pin 1)))
    (net (code 52) (name "Net-(D5-Pad1)")
      (node (ref D5) (pin 1))
      (node (ref U7) (pin 7)))
    (net (code 53) (name "Net-(R24-Pad1)")
      (node (ref U6) (pin 2))
      (node (ref R26) (pin 1))
      (node (ref R36) (pin 1))
      (node (ref R25) (pin 1))
      (node (ref R35) (pin 1))
      (node (ref R24) (pin 1)))
    (net (code 54) (name "Net-(R28-Pad2)")
      (node (ref R28) (pin 2))
      (node (ref SW3) (pin 8)))
    (net (code 55) (name "Net-(R27-Pad2)")
      (node (ref SW3) (pin 10))
      (node (ref R27) (pin 2)))
    (net (code 56) (name "Net-(R37-Pad2)")
      (node (ref SW3) (pin 9))
      (node (ref R37) (pin 2)))
    (net (code 57) (name "Net-(R38-Pad2)")
      (node (ref R38) (pin 2))
      (node (ref SW3) (pin 7)))
    (net (code 58) (name "Net-(R27-Pad1)")
      (node (ref U7) (pin 2))
      (node (ref R27) (pin 1))
      (node (ref R29) (pin 1))
      (node (ref R38) (pin 1))
      (node (ref R37) (pin 1))
      (node (ref R28) (pin 1)))
    (net (code 59) (name "Net-(R29-Pad2)")
      (node (ref R29) (pin 2))
      (node (ref SW3) (pin 6)))
    (net (code 60) (name "Net-(R21-Pad2)")
      (node (ref R21) (pin 2))
      (node (ref SW1) (pin 10)))
    (net (code 61) (name "Net-(R33-Pad2)")
      (node (ref R33) (pin 2))
      (node (ref SW1) (pin 9)))
    (net (code 62) (name "Net-(R22-Pad2)")
      (node (ref R22) (pin 2))
      (node (ref SW1) (pin 8)))
    (net (code 63) (name "Net-(R34-Pad2)")
      (node (ref SW1) (pin 7))
      (node (ref R34) (pin 2)))
    (net (code 64) (name "Net-(R21-Pad1)")
      (node (ref R34) (pin 1))
      (node (ref R33) (pin 1))
      (node (ref R23) (pin 1))
      (node (ref R21) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref R22) (pin 1)))
    (net (code 65) (name "Net-(R23-Pad2)")
      (node (ref SW1) (pin 6))
      (node (ref R23) (pin 2)))
    (net (code 66) (name "Net-(R24-Pad2)")
      (node (ref SW2) (pin 10))
      (node (ref R24) (pin 2)))
    (net (code 67) (name "Net-(R35-Pad2)")
      (node (ref R35) (pin 2))
      (node (ref SW2) (pin 9)))
    (net (code 68) (name "Net-(R25-Pad2)")
      (node (ref R25) (pin 2))
      (node (ref SW2) (pin 8)))
    (net (code 69) (name "Net-(R36-Pad2)")
      (node (ref SW2) (pin 7))
      (node (ref R36) (pin 2)))
    (net (code 70) (name "Net-(R26-Pad2)")
      (node (ref SW2) (pin 6))
      (node (ref R26) (pin 2)))
    (net (code 71) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2)))
    (net (code 72) (name "Net-(J4-Pad3)")
      (node (ref J4) (pin 3)))
    (net (code 73) (name "Net-(J4-Pad4)")
      (node (ref J4) (pin 4)))
    (net (code 74) (name "Net-(J4-Pad6)")
      (node (ref J4) (pin 6)))
    (net (code 75) (name "Net-(D1-Pad2)")
      (node (ref R47) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 76) (name "Net-(D2-Pad2)")
      (node (ref R48) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 77) (name Ain04)
      (node (ref U4) (pin 12))
      (node (ref R14) (pin 2))
      (node (ref R18) (pin 2)))
    (net (code 78) (name Vbat04)
      (node (ref J14) (pin 2))
      (node (ref J15) (pin 2))
      (node (ref U8) (pin 5))
      (node (ref J9) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 79) (name Vbat02)
      (node (ref R12) (pin 1))
      (node (ref J7) (pin 2))
      (node (ref J13) (pin 2))
      (node (ref U6) (pin 5))
      (node (ref J12) (pin 2)))
    (net (code 80) (name Vbat03)
      (node (ref J17) (pin 2))
      (node (ref J16) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref J8) (pin 2))
      (node (ref U7) (pin 5)))
    (net (code 81) (name SCL)
      (node (ref J2) (pin 3))
      (node (ref U3) (pin 20)))
    (net (code 82) (name Vbat01)
      (node (ref J6) (pin 2))
      (node (ref U5) (pin 5))
      (node (ref R11) (pin 1))
      (node (ref J10) (pin 2))
      (node (ref J11) (pin 2)))
    (net (code 83) (name Ain02)
      (node (ref R16) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref U4) (pin 14)))
    (net (code 84) (name SDA)
      (node (ref J2) (pin 4))
      (node (ref U3) (pin 19)))
    (net (code 85) (name Ain03)
      (node (ref R13) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref U4) (pin 15)))
    (net (code 86) (name Z)
      (node (ref U3) (pin 15))
      (node (ref U4) (pin 3)))
    (net (code 87) (name Ain01)
      (node (ref R11) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref U4) (pin 13)))
    (net (code 88) (name "Net-(R30-Pad2)")
      (node (ref R30) (pin 2))
      (node (ref SW4) (pin 10)))
    (net (code 89) (name "Net-(R39-Pad2)")
      (node (ref R39) (pin 2))
      (node (ref SW4) (pin 9)))
    (net (code 90) (name "Net-(R31-Pad2)")
      (node (ref R31) (pin 2))
      (node (ref SW4) (pin 8)))
    (net (code 91) (name "Net-(R40-Pad2)")
      (node (ref R40) (pin 2))
      (node (ref SW4) (pin 7)))
    (net (code 92) (name "Net-(R30-Pad1)")
      (node (ref R32) (pin 1))
      (node (ref U8) (pin 2))
      (node (ref R30) (pin 1))
      (node (ref R39) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref R40) (pin 1)))
    (net (code 93) (name "Net-(R32-Pad2)")
      (node (ref SW4) (pin 6))
      (node (ref R32) (pin 2)))
    (net (code 94) (name "Net-(D5-Pad2)")
      (node (ref D5) (pin 2))
      (node (ref R51) (pin 2)))
    (net (code 95) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref R52) (pin 2)))
    (net (code 96) (name "Net-(D8-Pad1)")
      (node (ref D8) (pin 1))
      (node (ref U8) (pin 6)))
    (net (code 97) (name "Net-(D7-Pad1)")
      (node (ref D7) (pin 1))
      (node (ref U8) (pin 7)))
    (net (code 98) (name "Net-(D7-Pad2)")
      (node (ref R53) (pin 2))
      (node (ref D7) (pin 2)))
    (net (code 99) (name "Net-(D8-Pad2)")
      (node (ref R54) (pin 2))
      (node (ref D8) (pin 2)))))