(export (version D)
  (design
    (source /home/hendrik/Schreibtisch/openReflow/Platine/openReflow.sch)
    (date "Sa 15 Sep 2018 11:41:34 CEST")
    (tool "Eeschema 5.0.0")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title SimpleReflowController)
        (company)
        (rev "Rev 1")
        (date 2018-08-17)
        (source openReflow.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref XA1)
      (value Arduino_Nano_Socket)
      (footprint Arduino:Arduino_Nano_Socket)
      (libsource (lib openReflow-rescue) (part Arduino_Nano_Socket) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B76F478))
    (comp (ref J4)
      (value TFT)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical)
      (libsource (lib openReflow-rescue) (part Conn_01x08) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B76F5FD))
    (comp (ref U4)
      (value MAX31855KASA)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib openReflow-rescue) (part MAX31855KASA) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B76FD74))
    (comp (ref J1)
      (value "Voltage Input 12V")
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal)
      (libsource (lib openReflow-rescue) (part Screw_Terminal_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B770027))
    (comp (ref U1)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (libsource (lib openReflow-rescue) (part LM1117-3.3) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B7702DA))
    (comp (ref U2)
      (value LM1117-5.0)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (libsource (lib openReflow-rescue) (part LM1117-5.0) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77035A))
    (comp (ref R3)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B770B1A))
    (comp (ref R4)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B770CDF))
    (comp (ref D3)
      (value LL4007)
      (footprint Diode_SMD:D_SMB)
      (libsource (lib openReflow-rescue) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B770FCE))
    (comp (ref D4)
      (value LL4007)
      (footprint Diode_SMD:D_SMB)
      (libsource (lib openReflow-rescue) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B7711FA))
    (comp (ref C6)
      (value 10nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B7718A9))
    (comp (ref J3)
      (value Temp2)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal)
      (libsource (lib openReflow-rescue) (part Screw_Terminal_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B771BCF))
    (comp (ref U3)
      (value MAX31855KASA)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib openReflow-rescue) (part MAX31855KASA) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B773001))
    (comp (ref R1)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77300A))
    (comp (ref R2)
      (value "10 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B773010))
    (comp (ref D1)
      (value LL4007)
      (footprint Diode_SMD:D_SMB)
      (libsource (lib openReflow-rescue) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B773017))
    (comp (ref C3)
      (value 10nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B773029))
    (comp (ref J2)
      (value Temp1)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal)
      (libsource (lib openReflow-rescue) (part Screw_Terminal_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77302F))
    (comp (ref J8)
      (value SSR-25DA_02)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal)
      (libsource (lib openReflow-rescue) (part Screw_Terminal_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B773B56))
    (comp (ref R7)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B773C69))
    (comp (ref J7)
      (value SSR-25DA_01)
      (footprint TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal)
      (libsource (lib openReflow-rescue) (part Screw_Terminal_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77496B))
    (comp (ref R5)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B774971))
    (comp (ref C1)
      (value 10µF)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-2012-12_Kemet-R)
      (libsource (lib openReflow-rescue) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77635B))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B776DE7))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B777134))
    (comp (ref J9)
      (value Servo)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib openReflow-rescue) (part Conn_01x03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B7799D9))
    (comp (ref J6)
      (value Status_LED)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib openReflow-rescue) (part Conn_01x03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77AC3E))
    (comp (ref R6)
      (value "1 kΩ")
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77BBDD))
    (comp (ref J10)
      (value Encoder)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (libsource (lib openReflow-rescue) (part Conn_01x04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77D771))
    (comp (ref D2)
      (value LL4007)
      (footprint Diode_SMD:D_SMB)
      (libsource (lib openReflow-rescue) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B77301D))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B782CD6))
    (comp (ref C7)
      (value 100nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib openReflow-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B78307B))
    (comp (ref J5)
      (value Buzzer)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib openReflow-rescue) (part Conn_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B783FF4))
    (comp (ref Q1)
      (value 2N3906)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BEC) (description "Transistor PNP (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9D4274))
    (comp (ref Q2)
      (value 2N3906)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BEC) (description "Transistor PNP (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9D453A))
    (comp (ref Q3)
      (value 2N3906)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BEC) (description "Transistor PNP (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9D45BE)))
  (libparts
    (libpart (lib Device) (part Q_PNP_BEC)
      (description "Transistor PNP (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PNP_BEC))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib openReflow-rescue) (part Arduino_Nano_Socket)
      (footprints
        (fp Arduino_Nano_Socket))
      (fields
        (field (name Reference) XA)
        (field (name Value) Arduino_Nano_Socket))
      (pins
        (pin (num 5V) (name 5V) (type power_in))
        (pin (num 3V3) (name 3.3V) (type power_in))
        (pin (num A0) (name A0) (type BiDi))
        (pin (num A1) (name A1) (type BiDi))
        (pin (num A2) (name A2) (type BiDi))
        (pin (num A3) (name A3) (type BiDi))
        (pin (num A4) (name A4_SDA) (type BiDi))
        (pin (num A5) (name A5_SCL) (type BiDi))
        (pin (num A6) (name A6) (type input))
        (pin (num A7) (name A7) (type input))
        (pin (num AREF) (name AREF) (type input))
        (pin (num D0) (name D0_RX0) (type BiDi))
        (pin (num D1) (name D1_TX0) (type BiDi))
        (pin (num D2) (name D2_INT0) (type BiDi))
        (pin (num D3) (name D3_INT1) (type BiDi))
        (pin (num D4) (name D4) (type BiDi))
        (pin (num D5) (name D5) (type BiDi))
        (pin (num D6) (name D6) (type BiDi))
        (pin (num D7) (name D7) (type BiDi))
        (pin (num D8) (name D8) (type BiDi))
        (pin (num D9) (name D9) (type BiDi))
        (pin (num D10) (name D10_CS) (type BiDi))
        (pin (num D11) (name D11_MOSI) (type BiDi))
        (pin (num D12) (name D12_MISO) (type BiDi))
        (pin (num D13) (name D13_SCK) (type BiDi))
        (pin (num GND1) (name GND) (type power_in))
        (pin (num GND2) (name GND) (type power_in))
        (pin (num RST1) (name RESET) (type openCol))
        (pin (num RST2) (name RESET) (type openCol))
        (pin (num VIN) (name VIN) (type power_in))))
    (libpart (lib openReflow-rescue) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib openReflow-rescue) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib openReflow-rescue) (part Conn_01x02)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib openReflow-rescue) (part Conn_01x03)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib openReflow-rescue) (part Conn_01x04)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib openReflow-rescue) (part Conn_01x08)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x08))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib openReflow-rescue) (part D)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib openReflow-rescue) (part LM1117-3.3)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-3.3))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib openReflow-rescue) (part LM1117-5.0)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-5.0))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib openReflow-rescue) (part MAX31855KASA)
      (footprints
        (fp SOIC*3.9x4.9mm*Pitch1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MAX31855KASA)
        (field (name Footprint) Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name T-) (type passive))
        (pin (num 3) (name T+) (type passive))
        (pin (num 4) (name VCC) (type power_in))
        (pin (num 5) (name SCK) (type input))
        (pin (num 6) (name ~CS~) (type input))
        (pin (num 7) (name SO) (type output))))
    (libpart (lib openReflow-rescue) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib openReflow-rescue) (part Screw_Terminal_01x02)
      (footprints
        (fp Connector*Terminal*Block*:*)
        (fp TerminalBlock*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive)))))
  (libraries
    (library (logical Device)
      (uri /home/hendrik/bin/KiCAD/V5.XX/kicad-symbols-master/Device.lib))
    (library (logical openReflow-rescue)
      (uri /home/hendrik/Tausch/openReflow/Platine/openReflow-rescue.lib)))
  (nets
    (net (code 1) (name "Net-(Q3-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref Q3) (pin 1)))
    (net (code 2) (name "Net-(J8-Pad1)")
      (node (ref J8) (pin 1))
      (node (ref Q3) (pin 3)))
    (net (code 3) (name "Net-(C3-Pad2)")
      (node (ref C3) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref U3) (pin 3)))
    (net (code 4) (name "Net-(C3-Pad1)")
      (node (ref U3) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref C3) (pin 1)))
    (net (code 5) (name "Net-(Q2-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 6) (name "Net-(J7-Pad1)")
      (node (ref J7) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 7) (name CS)
      (node (ref J4) (pin 6))
      (node (ref XA1) (pin D10)))
    (net (code 8) (name "Net-(D3-Pad2)")
      (node (ref U4) (pin 5))
      (node (ref R4) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 9) (name MISO)
      (node (ref XA1) (pin D12))
      (node (ref U3) (pin 7))
      (node (ref U4) (pin 7)))
    (net (code 10) (name VIN)
      (node (ref C1) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 3)))
    (net (code 11) (name SDA)
      (node (ref XA1) (pin A4))
      (node (ref J4) (pin 3)))
    (net (code 12) (name DC)
      (node (ref J4) (pin 4))
      (node (ref XA1) (pin D9)))
    (net (code 13) (name RESET_TFT)
      (node (ref J4) (pin 5))
      (node (ref XA1) (pin D8)))
    (net (code 14) (name 5V)
      (node (ref Q3) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref J4) (pin 8))
      (node (ref C5) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref J9) (pin 2))
      (node (ref XA1) (pin 5V))
      (node (ref J6) (pin 2)))
    (net (code 15) (name "Net-(D2-Pad2)")
      (node (ref U3) (pin 6))
      (node (ref D2) (pin 2))
      (node (ref R1) (pin 2)))
    (net (code 16) (name "Net-(D1-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref U3) (pin 5)))
    (net (code 17) (name 3V3)
      (node (ref R3) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U3) (pin 4))
      (node (ref J4) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref U4) (pin 4)))
    (net (code 18) (name GND)
      (node (ref J10) (pin 4))
      (node (ref J8) (pin 2))
      (node (ref J7) (pin 2))
      (node (ref XA1) (pin GND2))
      (node (ref XA1) (pin GND1))
      (node (ref J6) (pin 3))
      (node (ref J9) (pin 3))
      (node (ref J4) (pin 7))
      (node (ref C5) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref J5) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 19) (name "Net-(C6-Pad2)")
      (node (ref J3) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref U4) (pin 3)))
    (net (code 20) (name "Net-(C6-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref U4) (pin 2)))
    (net (code 21) (name SCK)
      (node (ref D3) (pin 1))
      (node (ref XA1) (pin D13))
      (node (ref D1) (pin 1))
      (node (ref J4) (pin 2)))
    (net (code 22) (name "Net-(J5-Pad2)")
      (node (ref Q1) (pin 3))
      (node (ref J5) (pin 2)))
    (net (code 23) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 24) (name "Net-(D4-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U4) (pin 6))
      (node (ref D4) (pin 2)))
    (net (code 25) (name SSR2)
      (node (ref R7) (pin 2))
      (node (ref XA1) (pin D5)))
    (net (code 26) (name Servo)
      (node (ref XA1) (pin D11))
      (node (ref J9) (pin 1)))
    (net (code 27) (name TC1_CS)
      (node (ref D2) (pin 1))
      (node (ref XA1) (pin D6)))
    (net (code 28) (name Status_LED)
      (node (ref XA1) (pin D3))
      (node (ref J6) (pin 1)))
    (net (code 29) (name SSR1)
      (node (ref XA1) (pin D4))
      (node (ref R5) (pin 2)))
    (net (code 30) (name A2)
      (node (ref J10) (pin 3))
      (node (ref XA1) (pin A2)))
    (net (code 31) (name TC2_CS)
      (node (ref XA1) (pin D7))
      (node (ref D4) (pin 1)))
    (net (code 32) (name A1)
      (node (ref J10) (pin 2))
      (node (ref XA1) (pin A1)))
    (net (code 33) (name A0)
      (node (ref XA1) (pin A0))
      (node (ref J10) (pin 1)))
    (net (code 34) (name Buzzer)
      (node (ref XA1) (pin D2))
      (node (ref R6) (pin 2)))
    (net (code 35) (name "Net-(XA1-PadD1)")
      (node (ref XA1) (pin D1)))
    (net (code 36) (name "Net-(XA1-PadD0)")
      (node (ref XA1) (pin D0)))
    (net (code 37) (name "Net-(XA1-PadAREF)")
      (node (ref XA1) (pin AREF)))
    (net (code 38) (name "Net-(XA1-PadA7)")
      (node (ref XA1) (pin A7)))
    (net (code 39) (name "Net-(XA1-PadA6)")
      (node (ref XA1) (pin A6)))
    (net (code 40) (name "Net-(XA1-PadA5)")
      (node (ref XA1) (pin A5)))
    (net (code 41) (name "Net-(XA1-PadA3)")
      (node (ref XA1) (pin A3)))
    (net (code 42) (name "Net-(XA1-PadVIN)")
      (node (ref XA1) (pin VIN)))
    (net (code 43) (name "Net-(XA1-PadRST2)")
      (node (ref XA1) (pin RST2)))
    (net (code 44) (name "Net-(XA1-PadRST1)")
      (node (ref XA1) (pin RST1)))
    (net (code 45) (name "Net-(XA1-Pad3V3)")
      (node (ref XA1) (pin 3V3)))))